

**RUGGED DIESEL EXHAUST FLUID**

ID# CRT-DEL-072611-00021

API LICENSE # 0102

|  |  |
| --- | --- |
| CAPACITY | 55 GALLON |
| FILL DATE | 7/18/2018 |
| DATE CODE | CP8-199 |



DEF

DEF

**Hazard Statement:**

None known

**Precautionary Statement**:

This material is not hazardous under the criteria of the Federal OSHA Hazard Communication Standard 29 CFR 1910.1200

**First Aid Statement**

First aid is not normally required. If breathing difficulties develop, move victim away from source of exposure and into fresh air in a position comfortable for breathing. Seek immediate medical attention.

If irritation or redness develops from exposure, flush eyes with clean water. If symptoms persist, seek medical attention.

Remove contaminated shoes and clothing and cleanse affected area(s) thoroughly by washing with mild soap and water or a waterless hand cleaner. If irritation or redness develops and persists, seek medical attention.

First aid is not normally required; however, if swallowed and symptoms develop, seek medical attention.

|  |  |
| --- | --- |
| **Health** | **1** |
| **Flammability** | **0** |
| **Reactivity** | **0** |
| **Personal Protection** |  |

***DOT SHIPPING NAME***

 Denver, CO. 80216

**(800)-580-4080**

**FOR HELP IN CHEMICAL**

**EMERGENCY**

**CALL CHEMTREC 800-424-9300**

BEFORE USING READ & UNDERSTAND CURRENT SDS FOR THIS PRODUCT

|  |
| --- |
| **ATTENTION:** |
| This container can present explosion or fire hazards, even when emptied! To avoid risk of injury, do not pressurize, cut, puncture or weld on or near this container. Since emptied containers retain product residue, follow label warnings even after container is emptied.  |